===================================================================================================================================================
  NEO Configurator:

- New features and change log.

===================================================================================================================================================

**** v3.4.0.0 (15/04/2026) *********************

* Compatible with firmware NEO+ v03.04.xx.04
* Compatible with firmware NEO v02.42.xx.42 
* No Compatible with NEO firmware prior to v02.40.xx.40

* Modifications and New Features:

  - EVAC Cloud and remote connection:
    - Support for the cloud Superadmin profile (same privileges as administrator or installer in the application).
	- Error message when connecting to an EVAC Core with an incompatible software version (lower than 1.2.0.0) while using the Superadmin profile.
    - Handling of multi-profile cloud accounts: ability to return to EVAC device selection and, from the system list, return to user selection.
    - Partner (account), subpartner, and user information in lists and the main window; with Manufacturer profile, an additional column shows each device’s
      partner and subpartner (Account).
    - System search filter is now case-insensitive.
    - The “Expired” field is no longer displayed in EVAC device lists because it is no longer in use.
  - ACSI triggers display "Any" when argument value 0 means any ACSI address or button.
  - Replaced "Cobranet" wording with "AES67" in texts related to NEO+ projects.
  - Replaced "Software reset" text with "Restart device" to avoid confusion with factory reset.
  - The last successfully logged-in user is remembered to autocomplete the start/login form (local and cloud connections).
  - OEM documentation: updated LEEME customization files with name variables for NEXO v1 and v2.

* Bug Fixes:

  - Fixed an issue that prevented adding AES67 streams in advanced mode.
  - Fixed an issue in zone and output name/description editing due to incorrect index parameters.
  - NEO DLL: fixed loss of ACSINet domain and zone group configuration (version 2.4.1.2); fixes for AES source deletion and AES67 source export with custom streams; error message
    when the maximum number of allowed custom AES streams is reached.
  - EVAC Cloud: fixed release of the remote connection endpoint on close; correct device connection state and "connected" state in EVAC Core device lists;
    filtering by partner and account name; loading flow for the list of accessible systems; cloud login process and displayed user information; brief UI
    freeze after the initial system list load; initial delay when applying the search filter; improvements to the cloud connection form and step-to-step flow.
  - Remote connection: fixes when taking into account the user uid and the EVAC Core software version.
  - Added Microsoft.Extensions.Logging.Abstractions dependency for cloud connection (Grpc.Net.Client / L4ToGrpcClient) and assembly binding redirects to resolve
    version conflicts with L4ToGrpcClient; L4ToGrpcClient subrepo update.
  - When going back from user selection with a multi-profile account, the login password field is cleared.
  - Invariant-culture string transformations independent of the application language; normalized cloud connection form strings in project resources.


**** v3.3.1.0 (02/07/2025) *********************

* Compatible with firmware NEO+ v03.03.xx.03
* Compatible with firmware NEO v02.42.xx.42 
* No Compatible with NEO firmware prior to v02.40.xx.40

* Modifications and New Features:

  - VAS Configurator (OEM): The EVAC Cloud logo is no longer shown by default. An option has been added to the OEM customization file to enable
    its display.

* Bug Fixes:

  - Fixed an issue where synchronization with devices would occasionally stop working permanently and requiring the application to be restarted to
    resolve the problem.



**** v3.3.0.0 (12/05/2025) *********************

* Compatible with firmware NEO+ v03.03.xx.03
* Compatible with firmware NEO v02.42.xx.42 
* No Compatible with NEO firmware prior to v02.40.xx.40

* Modifications and New Features:

  - Master Backup configuration for NEO+ systems.
  - New functions to save and load NEO+ device presets from file  (firmware v03.03.xx.03).
  - Changes in the configuration of audio and control VLAN identifiers:
      - Editing through a new pop-up window.
      - In online mode, possibility to apply the configuration to selected devices or to the entire system.
      - During the system configuration export, the VLAN configuration is applied at the end of the process, with the result shown in the export report.

* Bug Fixes:

  - Fixed an issue where duplicate devices sometimes appeared in the list of found devices within the device search window.
  - Fixed an issue where device assignment was sometimes not displayed correctly in the device search window.
  - Fixed some issues that could cause the application to crash unexpectedly.
  - VAS Configurator (OEM): Fixed an issue where the custom logo for the OEM version of NEO+ was not copied correctly during installation.
  - VAS Configurator (OEM): Fixed an issue where custom names of OEM devices were not displayed correctly in the report generated after exporting the system configuration.




**** v3.2.1.1 (26/03/2025) *********************

* Compatible with firmware NEO+ v03.02.xx.02
* Compatible with firmware NEO v02.42.xx.42 
* Not compatible with NEO firmware prior to v02.40.xx.40

* Modifications and New Features:

  - The factory reset button is disabled for NEO+ devices in the device search window, as this function is not available for these models via the search protocol.

* Bug Fixes:

  - Fixed an issue where multiple devices were sometimes displayed alternately on the same line in the list of found devices within the device search window.
  - Fixed an issue where an external device’s IP address change could cause unintended effects on project devices.
  - Fixed an issue where downloading files from NEO+ devices frequently generated errors that prevented the download, especially with large files and/or slow connections.
  - Fixed an bug that occasionally caused the application to crash after exporting a project with an error result in the ACSI configuration.
  - VAS Configurator (OEM): Removed the LDA logo from the main window in the OEM version.
  - VAS Configurator (OEM): Fixed an issue that prevented the assignment of OEM devices in the device search window.
  - VAS Configurator (OEM): Fixed an issue where custom names of OEM ACSI devices were not displayed correctly.


**** v3.2.1.0 (16/01/2025) *********************

* Compatible with NEO+ firmware v03.02.xx.02
* Compatible with NEO firmware v02.42.xx.42 
* Not compatible with NEO firmware prior to v02.40.xx.40 

* Modifications and New Features:

  - Audio and control VLAN identifiers can have the same value on NEO+ devices

* Bug Fixes:

  - Fixed a bug that prevented audio input and output vu-meters from being read correctly on NEO+ projects.
  - Fixed a bug that prevented to correctly activate the button to add new ACSI devices in the ACSI device configuration editor in NEO projects.
  - Fixed a bug that prevented the change from an ACSI device model to MPS8Z+ from being displayed correctly.
  - The default value for the “Enable All-Call PTT in PA Mode” and “Enable All-Call PTT in VA Mode” parameters is corrected by setting it to true (yes).
  


**** v3.2.0.0 (29/11/2024) *********************

* Compatible with NEO+ firmware v03.02.XX.02
* Compatible with NEO firmware v02.42.XX.42 
* Not compatible with NEO firmware prior to v02.40.XX.40 

* Modifications and New Features:

  - ACSINet Domain configuration.
  - All users profiles can "import systems" from the device discovery window.
  
  

**** v3.1.0.0 (29/11/2024) *********************

* Compatible with NEO+ firmware v03.02.XX.02
* Compatible with NEO firmware v02.42.XX.42 
* Not compatible with NEO firmware prior to v02.40.XX.40 

* Modifications and New Features:

  - Integration with NEO+ devices:
    - Configuration for AES67 audio reception and transmission.
    - Link loop monitoring (Port B) in the System Controller (advanced configuration).
  - Integration with EVAC Cloud for remote configuration of NEO and NEO+ systems.
  - Compatibility with existing projects from NEO Configurator v2.42.X.X

* Bug Fixes:

  - Fixed various issues causing unexpected application closing. 



**** v2.42.2.0 (24/11/2023) *********************

* Compatible with NEO firmware v02.42.XX.42
* Not compatible with NEO firmware prior to v02.40.XX.40

* Bug Fixes:
  - Fixed a bug in the configuration of delays and advanced equalization parameters for four-channel devices.



**** v2.42.1.0 (07/08/2023) *********************

* Compatible with firmware v02.42.XX.42.
* Not compatible with firmware prior to v02.40.XX.40.

* Modifications and New Features:
  - Added ACSI devices model MPS8Z+




**** v2.42.0.0 (07/07/2023) *********************

* Compatible with firmware v02.42.XX.42.
* Not compatible with firmware prior to v02.40.XX.40.

* Modifications and New Features:

  - Installer is now compatible with ARM64 architectures.
  - Added warning for "event edit mode is open" when importing from the "Search Devices" window.
  - Added warning for "project parameter will be overwritten" when importing a system from the "Search Devices" window.
  - When changing the "Enable Digital Audio Link Supervision" parameter on the Master, it prompts whether to apply
    the same value to the Extensions.
  - Changing the "Enable Digital Audio Link Supervision" parameter on an Extension only applies to that device.
  - Added new entry 'Internal AC/DC Power' in the Status Inputs and Outputs for every NEO device (Controller and
    Extensions) for monitoring of the Main Power (AC) and Emergency Power (DC) inputs.

* Bug Fixes:

  - Fixed an issue where values for PA and VA compatibility flags in Triggers, Conditions, and Actions were not
    displayed correctly.
  - Interface corrections to properly display texts in different controls.
  - Fixed an issue where the main application window was not displayed when opening on a secondary monitor.
  - Allowed "Execute Other Actions" actions to repeat actions in their execution sequence.
  - Fixed maximum character size for Command-type actions and triggers in hexadecimal format (twice the characters as
    ASCII format since 1 byte = two hexadecimal digits).
  - Fixed maximum size for UDP Command type actions (54 characters) and 485 Command type actions (60 characters).
  - Fixed an issue where the warning dialogue about NEO devices having a higher firmware version than expected was not
    fully displayed.
	




**** v2.41.0.0 (13/04/2023) *********************

* Compatible with firmware v02.41.XX.40
* No Compatible with firmware versions prior to v02.40.XX.40

* Changes:

  - Added advanced parameter setting "Enable Digital Audio Link Supervision" for NEO Controller and Extensions.
  - Added "identify" function for ACSIv2 devices found with the device discover window.
  - ACSI devices found with the device discover window can now be added to the project from there.
  
* Bug fixes:

  - Fixed a bug where sometimes the main toolbar for editing events remained incorrectly visible in unrelated configuration
    panels of the application.
  - Corrections to the Russian translation.





**** v2.40.0.3 (31/01/2023) *********************

* Compatible with firmware v02.40.XX.40
* No Compatible with firmware versions prior to v02.40.XX.40

* Bug fixes:

  - Fixed a bug where output channels corresponding to NEO Extensions were sometimes incorrectly displayed in red.
  - The project PDF report generation function has been modified to display correctly in all languages.
  - Device assignment in the Discover window has been corrected as it sometimes did not work correctly depending on the language configured in the app.
  - Corrections to the Russian translation.




**** v2.40.0.2 (1/08/2022) *********************

* Compatible with firmware v02.40.XX.40
* No Compatible with firmware versions prior to v02.40.XX.40

* Changes:

  - Name change: ACSI VAP1DE devices are now called VAP1FES.
  - Corrections to the Russian translation.




**** v2.40.0.1 (06/07/2022) *********************

* Compatible with firmware v02.40.XX.40
* No Compatible with firmware versions prior to v02.40.XX.40

* Bug fixes:

  - Fixed a bug that prevented from correctly showing connection status of ACSI V2 devices in the System Devices view tree.




**** v2.40.0.0 (01/07/2022) *********************

* Compatible with firmware v02.40.XX.40
* No Compatible with firmware versions prior to v02.40.XX.40

* Changes and new functionality:

  - Now its possible to select the filter type for audio input and output equalizers: Peaking, Low Pass, High Pass, Low-Shelf, Hi-Shelf,
    Low Pass Butterworth, High Pass Butterworth y Coeficientes IIR (this one only available for audio outputs).
  - Zone Groups configuration.
  - ACSI devices configuration has been updated to acommodate the new ACSIv2 protocol and the ACSIv1 protocol upgrade:
    + When a project saved with a previous version of NEO Configurator is opened the stored ACSI configuration will be lost due to incompatibility
      issues. A message warning of this circumstance will be shown while opening a project.
    + With the new and upgraded ACSI protocols we are now able to do the following:
      * Configure individual supervision for all ACSI devices.
      * Configure custom priority that overrides default ACSI address priority.
      * Disable ACSI bus autodetect functionality (plug and play).
      * Assign a zone or group to each button of every ACSI device. A button can address all system zones or all system groups. A button
        assignment can be disabled (the button doesn't address any zone or group).
      * Configure up to 32 ACSI devices with ACSIv2 bus mode (ACSIv1 still only allows a maximum of 8 devices).
  - System views; 'PA Microphones' and 'E Microphones' nodes have been unified into the new 'ACSI Devices' node.
  - Configurable audio output delays for 4 channel extension devices.
  - Added "All-Call PTT" configuration (selectable independently for PA and VA).
  - Zonal and General ECI inputs can now be enabled/disabled.
  - Added new action in Event Manager to activate/deactivate external device faults.
  - Logs saved in txt format now includes a header with extended info of the device, such as serial number, MAC address, device model or firmware version.
  - A warning message will be displayed if you try to close the application, close the project or go to offline mode while an audio transfer is still active.




**** v2.30.0.0 (01/07/2022) *********************

* Compatible with firmware v02.30.XX.31
* No Compatible with firmware v02.40.XX.40 o higher

* Changes and new functionality:

  - Slovak and russian languages added.
  - New parameter for enabling/disabling the delay mode for joining to ECI fired VA messages playback from their start (Status Inputs and Outputs).
  - It is now possible to disable the Devices Factory Reset previous to the exporting process by means of a checkbox in the confirmation exporting dialog.
  - When exporting a project to the system devices:
    + If there is no connection with the System Controller the process will be aborted.
    + If there is no connection with some Extension device, we are prompted to choose to continue if we want to proceed anyway (system will not be 100%
      configured).
    + If any device has a not compatible firmware version the process will be aborted.
    + If the System Controller and the Extensions don't have all the same firmware version the process will be aborted.
  
* Bug fixes:

  - Fixed a bug that prevented the user from opening firmware files with ".bin" extension when the application was configured in turkish language.
  - Fixed a bug that prevented the user from performing firmware updates ('Update' button didn't work) when the application was configured in certain languages.




**** v0.2.5.4 (17/02/2020) *********************

 * Compatibility with firmware v02.28.XX.30 (backwards compatible only with firmware v02.27.XX.29).

 * Modifications and New Functions:

   - PA view and VA view are now unified under the new "PA/VA view".

   - Event manager:
      + New Edition Mode (for NEO Firmware v02.28.XX.30 or higher).
      + Actions "Load events from file...", "Save event to file..." and "Delete all events" are now moved into the Events Editor bar and will be only active during the "Edit Events" mode.

   - Speaker Lines supervision
     + Support for the new "Class A" and "A+B" modes, and "Protection System".
     + "Low accuracy" status renamed as "Out of Range V - I"
     + "Not Valid" status in A+B mode applies to the whole line, not the branch.
     + "Not Valid" and "Bad Calibration" are shown if any branch is protected.
     + "EOL inputs" column placed between "Line status" and "Imp. Meas."
     + Modifed texts:
       * "EOL inputs" changed to "EOL Inputs (TFL1)"
       * "Imp. Meas." changed to "Impedance Measure (TFL2)"
       * "Protect" changed to "Protection System (TFL2)"
       * "Impedance" changed to "Measured Impedance"
       * "Imp. Dev." changed to "Impedance Deviation"
       * "Imp. Lower Tol" changed to "Impedance Lower Tolerance"
       * "Imp. Upper Tol" changed to "Impedance Upper Tolerance"
     + "Impedance Measure (TFL2)" column now allows 2 new methods: "A+B Mode" and "Class A" (loop from A to B).
     + Systems with firmare older than v02.28.XX.30 will show only the options "None" and "Single Line" in the "Impedance Measure (TFL2)" column.    

   - Logs:
     + "Device Log" now visible in profile "Installer".
     + All logs are available in the root of the "Device" view tree.
     + EMG, FLT and DIS logs include the full log (both active and solved entries).
     + Column "Id" now renamed as "Flexnet Id". This makes reference to the device ID which the logs belongs to.
     + Full logs are shown by default (parameter "days" equal to 0).
     + When saving logs, the default format will be "txt".

   - Power Amplifier Outputs:
     + Title "Amplfier Channels" changed into "Power Amplifier Outputs".
     + "Mute" column renamed to "Output Mute"
     + Added "Zone Mute" column (only reading).


   - Removed the list of zones within the tree of the "PA/VA view".   

   - Added configuration for PA and VA volumes in ACSI microphones.   

   - "Enable Overrides with PA Mics" text modified to "Enable Overrides and VA Volumes with PA Mics".

   - Removed "Default Configuration" button from Zones configuration.

   - Search Devices window: 
     + Button "Update" text changed to "Refresh". 
     + Button "IP range" text changed to "Filer by IP".
     + Added confirmation when trying to change the IP of a device.

   - New error message "ACSI device not found" when trying to update an ACSI devices which is not currently connected to the Master unit.

   - New warning: when removing master unit, a dialog window will warn that all the configuration will be lost if the master unit is removed.

   - PDF report updated to show the new features.

   - Updated translations for Spanish, French, German, Italian and Turkish.
   
 
 * Bug fixes.
  
  - Datagrid is now shown correctly after redimensioning the window.
  
  - ACSI Extension keyboards physically connected are properly shown in green in NEO Configurator. 

  - The profile "Maintainer" can no longer remove (or add) VA microphones. 

  - Amplifier Outputs: supervision activation parameter is refreshed correctly now. 

  - Search Devices window: 
    + Search devices function is now working properly when filering by IP.
    + The selected device in the top area is not lost when data is refreshed.

  - ACSI devices firmware update: "Invalid arguments" error solved.

  - Events:
     + Change of name/description of "Delay" actions now working properly.
     + ACSI triggers now appear correctly under "Conditions".
     + Exporting events into file functions exports the events as shown in the software (not the events loaded in the physical system).
     + Wrong IP or port parameters within UDP commands do not cause an unexpected close.

  - Scroll bars are now shown correctly in all configuration lists.
  - Speaker Lines: 
     + Impedance measurements do not disappear after each measurement.
     + Line supervision parameters have the same behaviour offline and online:
        * Enabling "EOL Inputs (TFL1)" will desable "Impedance Measure (TFL2)" and "Protection System (TFL2)".
        * Enabling any mode in "Impedance Measure (TFL2)" will also enable "Protection System (TFL2)" and disable "EOL Inputs (TFL1)".
        * "Protecion System (TFL2)" can only be enabled if any mode in "Impedance Measure (TFL2)" is also enabled.
     + "Protection System (TFL2)" is exported correctly to the physical system.

  - Fixed bug that did not allow to download system logs after uploading audio files.

  - Other minor bug fixes.

* IMPORTANT NOTICE: Project files created with this version cannot be opened with older versions.

***************************************************************************************************************************************************



**** v0.2.4.3 (19/02/2020) *********************

  - Added turkish language.

***************************************************************************************************************************************************




**** v0.2.4.2 (26/11/2019) *********************

  * Compatible with firmware up to version v02.27.XX.29

  * Bug fixes:

    - Fixed bug in checking the date and time of the NEO Master when importing / exporting the system configuration.

    - French text corrected for options for enabling the use of PA sources and microphones in VA mode..

    - Fixed bug in checking "hidden" parameters not saved in projects generated with versions prior to v0.2.3.0, specifically the parameters Z_HW_MIN and Z_HW_MAX did not receive the corresponding default values ​​according to the device model.

    - "Invalid" source routing are now corrected when saving, opening or exporting / importing a project (routing of hidden sources, audio message players, PTT or source 5 with ACSI devices installed or ACSI mode active when in Online mode).

    - Fixed bug that could cause an unexpected application crash during the project export process.

    - Fixed bug where, when opening projects prior to v0.2.3.0, the default values of the temperature monitoring "hidden" parameters for NEO8250E device models were not established.

    - Fixed bug that prevented from correctly editing the name of the first message in the list of prerecorded messages.

    - Fixed bug that prevented from correctly editing the screensaver parameters.

    - Fixed bug that prevented from correctly editing volume change actions (events).

    - Changes in events and conditions are now correctly updated when editing event and condition type triggers.

    - The first keypress of a valid character is now written directly in numeric type cells so you don't have to make two keypresses in order to write the first digit.

    - Fixed bug that prevented from correctly editing the first row in the Cobranet sources list.

    - Fixed bug in numerical type cells located in the last row of a list of parameters that sometimes forced a value to be entered twice to confirm it.

    - Fixed bug that prevented from correctly editing Cobranet Broadcast parameters when the project included NEO4500LE devices.

    - Devices search window: Fixed refresh of the VCC devices displayed on the project equipment when the system controller assignment is changed.

  * Changes:

    - Button text for speaker line calibration has been changed so it now describes its function better.

    - Firmware update window: Added model and IP filters. Added IP change and factory reset functions as in the devices search window.

    - Devices search window: Some unnecessary connections with found system controllers have been removed. These connections were, in some cases, the reason of connectivity problems with the project system controller.

    - Devices search window and Firmware update window: It is now possible to select only the first address of the IP filter. This allows performing a unicast search and check if there is any equipment at the specified address. Useful in case the network configuration does not allow bradcast traffic.

    - Improvements in parameter lists edition (some already included in previous versions):
      * Spacebar starts editing a cell without deleting current value or enables/disables a checkbox type cell.
      * 'Enter' key confirms the edited value and moves to the cell below.
      * 'Tab' key confirms value and moves to the cell to the right (or first cell in next row if the current cell is the last one in the row).
      * Pressing any valid character starts editing a cell (if editable) overwriting previous value.
      * 'Esc' key cancels editing a cell and restores previous value.

  * New features:

    - German and italian languages added.

    - A 'factory reset' of project devices is performed at the beginning of the project export process so that devices always get factory defaults before system configuration starts.

    - A 'soft reset' of project devices is performed after the project export process is finished (if there is no cancellation) so that the new system configuration starts working from clean state.

***************************************************************************************************************************************************




**** v0.2.4.1 (18/07/2019) *********************

  * Compatible with firmware up to version v02.27.XX.29

  * Bug fixes:

    - Fixed bug whereby when exporting a project to the NEO in which the impedance monitoring flag of a line is enabled, the value of the nominal impedance sent for said line was later overwritten since the enabling of said flag automatically programmed an impedance calibration for that line.

  * New features:

    - Now it is possible to import events from file while the application in offline mode.

    - New configurable parameters:

        + N/C mode for general and zonal CIE inputs (Controller and Extensions)
        + CIE Auto-Reset (Controller only)
        + Rec-Out active high (Controller only)
        + Status-Out: N/C and FLT/DIS mode configuration.
    
        These parameters have been incorporated in the section "Status Inputs" (now "Status Inputs and Outputs") of each equipment in the "System devices" view.

***************************************************************************************************************************************************




**** v0.2.3.1 (18/07/2019) *********************

    - Fixed bug introduced with version v0.2.3.0 by which actions for display calibration and front panel SD card formatting have disappeared from the "Advanced" section of the System Controller.

***************************************************************************************************************************************************




**** v0.2.3.0 (17/06/2019) *********************

  * Compatible with firmware up to version v02.26.xx.28 build 9.6

  * Bug fixes:

    - VAS Configurator: Fixed a bug that prevented the use of custom model strings for NEO Extensions.

    - Fixed "Name" column header text in Action List.

    - Fixed a bug that prevented the use of Event triggers in VA Events (online mode only).

    - Fixed a bug that caused an application crash when cancelling the "Save as" dialog opened after "Download project backup file" is selected in Tools menu.

    - Bug fixes in the "Discover" tool to solve some unexpected crashes of the application.

    - LOGS: Fixed a bug that caused an application crash when a too large value was entered in the "duration / days" fields.

    - Fixed a bug that prevented, in some cases, firmware updates for ACSI devices.

    - Fixed the synchronization of power amplification output gain values when, in online mode, they are remotely changed.

    - Now any editing key can activate edit mode in editable cells when they are selected (not only spacebar or mouse double-click).

    - Fixed a bug in screensaver configuration (Controller/Advanced).

    - Waiting dialog is now properly displayed when creating, opening, saving or closing projects.

  * Changes:

    - System Devices / Controllers node text has changed to "Controller".

    - System Devices / Controller / Audio Inputs : header text for column "LSE" has changed to "Sound Enhancer".

    - Read only checkboxes doesn't show square around the selection tick.

    - Removed the suffix "_copy" when duplicating events, triggers, conditions and actions.

    - EMG, FLT and DIS logs are now accesible from System Controller node too.

    - "Enable Port X Audio on EMG" and "Enable Port X Data on EMG" options are now located at VA View root node/Configuration/General instead of System Controller/Flexnet.

    - Data cells in parameter lists now adjust their height according to their content and width to show all content.

    - Zone lists: Column "N. Channels" text changed to "Power Amplifier Outputs" and now shows all the IDs of the Power Amplifier Outputs assigned to the zone.

    - Default priority value for New Events is now 50 for PA Events and 10 for VA Events.

    - Removed "Replace" button from Event, Trigger, Condition and Action lists.

    - Speaker Lines: "EOL" column is now divided in two checkbox columns; "EOL A" and "EOL B".

    - Speaker Lines: "Imp.Meas" is now a checkbox column.

  * New features:

    - 'PA Serial Port' and 'VA Serial Port' configuration added in Controller/Serial Ports

    - 'Disable System Beep' option added in Controller/Advanced.

    - 'Enable Subnet Broadcast Mode' option added in Controller/Flexnet.

  *** IMPORTANT:

    - With this version of the application certain parameters of the system are saved in the NEO Configurator projects and are likely to be exported to and imported from system devices, even though they are not visible in the application:

        * Conductor Priority
        * Disable Dinamic Limiters
        * Disable CM2 Supervision
        * Supervision - Common Parameters:
            - Tone Volume
            - Tone Freq
            - Tone Interval
            - Min Signal
            - Min Accuracy
        * Supervision - Amplifier Supervision:
            - Gain Tolerance
            - T. Error Th.
            - T. Lower Th.
            - T Higher Th. 
        * Supervision - CIE Interface Configuration
	    - Enable Input General
            - Enable Input Zones
        * Supervision - Line Supervision (EOL):
            - Fake Activation threshold
        * Supervision - Line Supervision (Z Meas):
            - Z HW Min
            - Z HW Max
            - V Min
            - V Max
            - I Min
            - I Max
        * Output Channels Noise Configuration:
            - Global Noise Generator - Noise Type
            - Mute Noise
            - Noise Level
        * Output Channels Filter Configuration (only in Extension devices):
            - Filter Enable
            - Filter Type
            - Filter Frequency
            - Filter Gain
            - Filter Boost
            - Filter Q Slope

    - It is important to keep this in mind when opening and exporting existing projects or when importing the configuration of a system with this version.

    - With new projects these parameters take the default values of the system (Factory defaults).

    - When opening projects generated with previous versions of the application, the default values will also be applied to those parameters, with the exception of:
            - Disable CM2 Supervision
            - Supervision CIE / Enable Input General
            - Supervision CIE / Enable Input Zones
            - Supervision - Common Parameters / Tone Volume
            - Supervision - Common Parameters / Tone Freq
            - Supervision - Common Parameters / Tone Interval
	    - Supervision - Line Supervision (EOL) / Fake Activation threshold
      whose values were already saved with the project but not exported.

***************************************************************************************************************************************************



**** v0.2.2.11 (13/03/2018) *********************

- Bug fix: Output backup channels can now be configured properly. (Bug introduced with version v0.2.2.10)

***************************************************************************************************************************************************



**** v0.2.2.10 (08/03/2018) *********************

- VAS Configurator - Bug fix: NEO Extensions can now be edited properly while in online mode (not showing model mismatch error when it does not apply).

- Bug fix: ACSI devices firmware updates are now working properly.

- Bug fix: Impedance measurement is now displayed correctly in NEO Extensions while in online mode.

- Fixed some icons in the "Search device" window.

- New button in "Start" window: FIRMWARE. A shortcut to the firmware updates window.

***************************************************************************************************************************************************



**** v0.2.2.9 (13/12/2017) *********************

- Added possibility to export events to file while in offline mode.

- VCCs are shown as "VCC-64" in the interface.

- Bug fix: buttons within "View" menu are shown in the proper language.

- Bug fix: NEO screensaver option is now working properly.

- Improved transmission of bundle firmware updates to NEO8060.

- Bug fix: frontal and ETX firmware updates can be sent separately to NEO8060 without reporting a model mismatch fault.

- The app is not crashing anymore when deleting/moving/renaming the file of an opened project.

- While exporting a project file in NEO, NEO will be in "maintenance mode": the PA led will be blinking and the touchscreen temporarily disabled until export is finished.

- New button in "Search Device" window: EXPORT SYSTEM.

- New button in "Search Device" window: UNLINK Extension Devices.

- Installation: The app will be installed by default in the same language selected during installation.

- VAS Configurator: The file 'company_icon.ico' within the folder '\CFG' will be used for the desktop shortcut and the start menu shortcut.

- Added feature to download and upload a backup file of the project within NEO8060 Internal Memory. This backup file is not modified if the configuration of NEO is changed. This file can be uploaded as an option into NEO Internal Memory whenver a Project file is being exported.

- The "Zone Editor" window now shows the custom name of the amplifier output instead of the generic name.

- "Search Device" window: all the NEO devices are shown in the Discover window, even if they are in the same network but in a different IP range. The devices in a different IP range will appear in red, showing that it is not possible to connect to them. Only the devices in the same IP range as the computer will appear in green, showing that they can be connected.

- Audio Files Fix:
  * WAV: They will always be sent to NEO even though Windows Media Player is not configured in the computer.
  * MP3: If there are no MP3 codecs in the system, a message error will be shown.

- Bug fix: the upload progress bar of audio files within the status bar is updated properly, even when the "Sending Audio Files" window is closed.

- Event Manager Bug Fix: It is now possible to edit volume level actions of audio sources when there is not Cobranet audio sourced defined in the system.

- Bug fix: The welcome page is displayed properly when a Windows Theme is using different sizes of fonts.

- Bug fix: It is not possible to add Extensions with "unknown" model anymore.

- Bug fix: the first trigger was always shown as inactive. Now it is shown properly as active or inactive.

- Text Corrections in French Language.
